Help Center -> Video device type

## Video device type

The new system video linkage function, to realize the management of the hard disk video recorder, real-time video view, video video query and linkage event happens to be automatic popup real-time video functions.

Use video linkage function, users need to advance in the equipment system in new network camera or hard disk video recorder, concrete operation please see Add Device. After completion of the new, users need to set up in linkage, set up corresponding video linkage action (pop-up video, video, paparazzi), one may use the video linkage function. Please refer to the specific Settings Linkage Settings.

Description: Only support the current version of the software in ZKTeco IPCameras and Hikvision (HIKVISION) embedded network DVR, DS-91xx Series, DS-81xx/71xx/72xxHV the series, DS-80xx/70xx/72xxH SeriesDS-78xx/88xx series, recommended model: HIK/DS-7808H-ST-AF-DVR-II-B/.8-4, other models, please contact Hikvision company and our company.